# PIP: Member List

PIBinaryLog Member List

This is the complete list of members for PIBinaryLog, including all inherited members.

canRead() const | PIIODevice | inlinevirtual
canWrite() const | PIIODevice | inlinevirtual
className() const | PIObject | inlinevirtual
clearThreadedWriteQueue() | PIIODevice | inline
close() | PIIODevice | inline
closed() | PIIODevice |
closeDevice() | PIBinaryLog | protectedvirtual
configure(const PIString &config_file, const PIString &section, bool parent_section=false) | PIIODevice |
configureDevice(const void *e_main, const void *e_parent=0) | PIIODevice | inlineprotectedvirtual
configureFromFullPath(const PIString &full_path) | PIBinaryLog | protectedvirtual
CONNECT | PIObject | related
CONNECT0 | PIObject | related
CONNECT1 | PIObject | related
CONNECT2 | PIObject | related
CONNECT3 | PIObject | related
CONNECT4 | PIObject | related
CONNECTU | PIObject | related
constructFullPath() const | PIBinaryLog | virtual
createFromFullPath(const PIString &full_path) | PIIODevice | static
createIndex() | PIBinaryLog |
createNewFile(const PIString &path) | PIBinaryLog |
createNewFile() | PIBinaryLog |
data() const | PIThread | inline
debug() const | PIObject | inline
defaultID() const | PIBinaryLog | inline
deleted() | PIObject | protected
DeviceMode enum name | PIIODevice |
DISCONNECT | PIObject | related
DISCONNECT0 | PIObject | related
DISCONNECT1 | PIObject | related
DISCONNECT2 | PIObject | related
DISCONNECT3 | PIObject | related
DISCONNECT4 | PIObject | related
emitter() const | PIObject | inlineprotected
EVENT | PIObject | related
EVENT0 | PIObject | related
EVENT1 | PIObject | related
EVENT2 | PIObject | related
EVENT3 | PIObject | related
EVENT4 | PIObject | related
EVENT_HANDLER | PIObject | related
EVENT_HANDLER0 | PIObject | related
EVENT_HANDLER1 | PIObject | related
EVENT_HANDLER2 | PIObject | related
EVENT_HANDLER3 | PIObject | related
EVENT_HANDLER4 | PIObject | related
EVENT_VHANDLER | PIObject | related
EVENT_VHANDLER0 | PIObject | related
EVENT_VHANDLER1 | PIObject | related
EVENT_VHANDLER2 | PIObject | related
EVENT_VHANDLER3 | PIObject | related
EVENT_VHANDLER4 | PIObject | related
fileEnd() | PIBinaryLog |
fileError() | PIBinaryLog |
filePrefix() const | PIBinaryLog | inline
filterID | PIBinaryLog |
findByName(const PIString &name) | PIObject | inlinestatic
flush() | PIIODevice | inlinevirtual
fullPathPrefix() const | PIBinaryLog | inlineprotectedvirtual
getLogInfo(const PIString &path) | PIBinaryLog | static
HANDLER | PIObject | related
init() | PIIODevice | inlineprotectedvirtual
initialize() | PIIODevice | inline
isClosed() const | PIIODevice | inline
isEmpty() const | PIBinaryLog | inline
isEnd() const | PIBinaryLog | inline
isOpened() const | PIIODevice | inline
isPropertyExists(const PIString &name) const | PIObject | inline
isReadable() const | PIIODevice | inline
isReopenEnabled() const | PIIODevice | inline
isRunning() const | PIThread | inline
isThreadedRead() const | PIIODevice | inline
isThreadedWrite() const | PIIODevice | inline
isWriteable() const | PIIODevice | inline
lastReadedID() const | PIBinaryLog | inline
lock() | PIThread | inline
logDir() const | PIBinaryLog | inline
logIndex() const | PIBinaryLog | inline
logInfo() const | PIBinaryLog | inline
logSize() const | PIBinaryLog | inline
mode() const | PIIODevice | inline
mutex() | PIThread | inline
name() const | PIObject | inline
needLockRun(bool need) | PIThread | inline
newFile(const PIString &filename) | PIBinaryLog |
open() | PIIODevice | inline
open(const PIString &_path) | PIIODevice | inline
open(const DeviceMode &_mode) | PIIODevice | inline
open(const PIString &_path, const DeviceMode &_mode) | PIIODevice | inline
openDevice() | PIBinaryLog | protectedvirtual
opened() | PIIODevice |
path() const | PIIODevice | inline
piCoutObj | PIObject | related
piDisconnect(PIObject *src, const PIString &sig) | PIObject | static
piDisconnect(PIObject *src) | PIObject | static
piHigh enum value | PIThread |
piHighest enum value | PIThread |
PIIODEVICE | PIIODevice | related
PIIODevice() | PIIODevice |
PIIODevice(const PIString &path, DeviceMode mode=ReadWrite) | PIIODevice |
piLow enum value | PIThread |
piLowerst enum value | PIThread |
piNormal enum value | PIThread |
PIObject(const PIString &name=PIString()) | PIObject |
PIOBJECT | PIObject | related
PIOBJECT_SUBCLASS | PIObject | related
PIThread(void *data, ThreadFunc func, bool startNow=false, int loop_delay=-1) | PIThread |
PIThread(bool startNow=false, int loop_delay=-1) | PIThread |
playDelay() const | PIBinaryLog | inline
playMode() const | PIBinaryLog | inline
PlayMode enum name | PIBinaryLog |
PlayRealTime enum value | PIBinaryLog |
playSpeed() const | PIBinaryLog | inline
PlayStaticDelay enum value | PIBinaryLog |
PlayVariableSpeed enum value | PIBinaryLog |
pos() const | PIBinaryLog | inline
Priority enum name | PIThread |
priority() const | PIThread | inline
properties() const | PIObject | inline
propertiesCount() const | PIObject | inline
property(const PIString &name) const | PIObject | inline
propertyChanged(const PIString &) | PIBinaryLog | protectedvirtual
rapidStart() const | PIBinaryLog | inline
read(void *read_to, int max_size) | PIBinaryLog | virtual
PIIODevice::read(int max_size) | PIIODevice | inline
readBinLog(int id=0, PISystemTime *time=0) | PIBinaryLog |
readBinLog(int id, void *read_to, int max_size, PISystemTime *time=0) | PIBinaryLog |
readDeviceSetting(const PIString &name, const T &def, const PIConfig::Entry *em, const PIConfig::Entry *ep) | PIIODevice | related
readForTime(double timeout_ms) | PIIODevice |
ReadOnly enum value | PIIODevice |
ReadWrite enum value | PIIODevice |
REGISTER_DEVICE | PIIODevice | related
reopenEnabled | PIIODevice |
reopenTimeout | PIIODevice |
reopenTimeout() | PIIODevice | inline
restart() | PIBinaryLog |
seek(const PISystemTime &time) | PIBinaryLog |
seekTo(int rindex) | PIBinaryLog |
setData(void *d) | PIThread | inline
setDebug(bool debug) | PIObject | inline
setDefaultID(int id) | PIBinaryLog | inline
setFilePrefix(const PIString &prefix) | PIBinaryLog | inline
setLogDir(const PIString &path) | PIBinaryLog | inline
setMode(DeviceMode m) | PIIODevice | inline
setName(const PIString &name) | PIObject | inline
setPath(const PIString &path) | PIIODevice | inline
setPlayDelay(const PISystemTime &delay) | PIBinaryLog | inline
setPlayMode(PlayMode mode) | PIBinaryLog | inline
setPlayRealTime() | PIBinaryLog | inline
setPlaySpeed(double speed) | PIBinaryLog | inline
setPriority(PIThread::Priority prior) | PIThread |
setProperty(const PIString &name, const PIVariant &value) | PIObject | inline
setRapidStart(bool enabled) | PIBinaryLog | inline
setReopenEnabled(bool yes=true) | PIIODevice | inline
setReopenTimeout(int msecs) | PIIODevice | inline
setSlot(ThreadFunc func) | PIThread | inline
setSplitFileSize(llong size) | PIBinaryLog | inline
setSplitMode(SplitMode mode) | PIBinaryLog | inline
setSplitRecordCount(int count) | PIBinaryLog | inline
setSplitTime(const PISystemTime &time) | PIBinaryLog | inline
setThreadedReadBufferSize(int new_size) | PIIODevice | inline
setThreadedReadData(void *d) | PIIODevice | inline
setThreadedReadSlot(ReadRetFunc func) | PIIODevice | inline
SplitCount enum value | PIBinaryLog |
splitFileSize() const | PIBinaryLog | inline
splitMode() const | PIBinaryLog | inline
SplitMode enum name | PIBinaryLog |
SplitNone enum value | PIBinaryLog |
splitRecordCount() const | PIBinaryLog | inline
SplitSize enum value | PIBinaryLog |
splitTime() const | PIBinaryLog | inline
SplitTime enum value | PIBinaryLog |
start() | PIIODevice | inline
PIThread::start(int timer_delay) | PIThread |
PIThread::start(ThreadFunc func, int timer_delay) | PIThread | inline
started() | PIThread |
startOnce() | PIThread |
startOnce(ThreadFunc func) | PIThread | inline
startThreadedRead() | PIIODevice | inline
startThreadedRead(ReadRetFunc func) | PIIODevice | inline
startThreadedWrite() | PIIODevice | inline
stop(bool wait=false) | PIIODevice | inline
stopped() | PIThread |
stopThreadedRead() | PIIODevice | inline
stopThreadedWrite() | PIIODevice | inline
superClassName() const | PIObject | inlinevirtual
threadedRead(uchar *readed, int size) | PIBinaryLog | protectedvirtual
threadedReadBuffer() const | PIIODevice | inline
threadedReadBufferSize | PIIODevice |
threadedReadBufferSize() const | PIIODevice | inline
threadedReadData() const | PIIODevice | inline
threadedReadEvent(uchar *readed, int size) | PIIODevice |
threadedWriteEvent(ullong id, int written_size) | PIIODevice |
unlock() | PIThread | inline
waitForFinish(int timeout_msecs) | PIThread |
waitForStart(int timeout_msecs) | PIThread |
WEAK_CONNECT | PIObject | related
WEAK_CONNECT0 | PIObject | related
WEAK_CONNECT1 | PIObject | related
WEAK_CONNECT2 | PIObject | related
WEAK_CONNECT3 | PIObject | related
WEAK_CONNECT4 | PIObject | related
write(const void *data, int size) | PIBinaryLog | inlinevirtual
PIIODevice::write(const PIByteArray &data) | PIIODevice | inline
writeBinLog(int id, PIByteArray data) | PIBinaryLog | inline
writeBinLog(int id, const void *data, int size) | PIBinaryLog |
writeBinLog_raw(int id, const PISystemTime &time, const PIByteArray &data) | PIBinaryLog | inline
writeCount() const | PIBinaryLog | inline
WriteOnly enum value | PIIODevice |
writeThreaded(const void *data, int max_size) | PIIODevice | inline
writeThreaded(const PIByteArray &data) | PIIODevice |