# PIP: Member List

PISerial Member List

This is the complete list of members for PISerial, including all inherited members.

availableDevices(bool test=false) | PISerial | static
availableSpeeds() | PISerial | static
canRead() const | PIIODevice | inlinevirtual
canWrite() const | PIIODevice | inlinevirtual
className() const | PIObject | inlinevirtual
clearThreadedWriteQueue() | PIIODevice | inline
close() | PIIODevice | inline
closed() | PIIODevice |
closeDevice() | PISerial | protectedvirtual
configure(const PIString &config_file, const PIString &section, bool parent_section=false) | PIIODevice |
configureDevice(const void *e_main, const void *e_parent=0) | PISerial | protectedvirtual
configureFromFullPath(const PIString &full_path) | PISerial | protectedvirtual
CONNECT | PIObject | related
CONNECT0 | PIObject | related
CONNECT1 | PIObject | related
CONNECT2 | PIObject | related
CONNECT3 | PIObject | related
CONNECT4 | PIObject | related
CONNECTU | PIObject | related
constructFullPath() const | PISerial | virtual
createFromFullPath(const PIString &full_path) | PIIODevice | static
data() const | PIThread | inline
dataBitsCount | PISerial |
dataBitsCount() const | PISerial | inline
debug() const | PIObject | inline
deleted() | PIObject | protected
device | PISerial |
device() const | PISerial | inline
DeviceMode enum name | PIIODevice |
DISCONNECT | PIObject | related
DISCONNECT0 | PIObject | related
DISCONNECT1 | PIObject | related
DISCONNECT2 | PIObject | related
DISCONNECT3 | PIObject | related
DISCONNECT4 | PIObject | related
emitter() const | PIObject | inlineprotected
EVENT | PIObject | related
EVENT0 | PIObject | related
EVENT1 | PIObject | related
EVENT2 | PIObject | related
EVENT3 | PIObject | related
EVENT4 | PIObject | related
EVENT_HANDLER | PIObject | related
EVENT_HANDLER0 | PIObject | related
EVENT_HANDLER1 | PIObject | related
EVENT_HANDLER2 | PIObject | related
EVENT_HANDLER3 | PIObject | related
EVENT_HANDLER4 | PIObject | related
EVENT_VHANDLER | PIObject | related
EVENT_VHANDLER0 | PIObject | related
EVENT_VHANDLER1 | PIObject | related
EVENT_VHANDLER2 | PIObject | related
EVENT_VHANDLER3 | PIObject | related
EVENT_VHANDLER4 | PIObject | related
findByName(const PIString &name) | PIObject | inlinestatic
flush() | PISerial | virtual
fullPathPrefix() const | PISerial | inlineprotectedvirtual
HANDLER | PIObject | related
init() | PIIODevice | inlineprotectedvirtual
initialize() | PIIODevice | inline
inSpeed() const | PISerial | inline
isClosed() const | PIIODevice | inline
isOpened() const | PIIODevice | inline
isParameterSet(PISerial::Parameters parameter) const | PISerial |
isPin(int number) const | PISerial |
isPropertyExists(const PIString &name) const | PIObject | inline
isReadable() const | PIIODevice | inline
isReopenEnabled() const | PIIODevice | inline
isRunning() const | PIThread | inline
isThreadedRead() const | PIIODevice | inline
isThreadedWrite() const | PIIODevice | inline
isWriteable() const | PIIODevice | inline
lock() | PIThread | inline
mode() const | PIIODevice | inline
mutex() | PIThread | inline
name() const | PIObject | inline
needLockRun(bool need) | PIThread | inline
open() | PIIODevice | inline
open(const PIString &_path) | PIIODevice | inline
open(const DeviceMode &_mode) | PIIODevice | inline
open(const PIString &_path, const DeviceMode &_mode) | PIIODevice | inline
openDevice() | PISerial | protectedvirtual
opened() | PIIODevice |
outSpeed() const | PISerial | inline
Parameters enum name | PISerial |
parameters() const | PISerial | inline
parityControl | PISerial |
ParityControl enum value | PISerial |
ParityOdd enum value | PISerial |
parityOdd | PISerial |
path() const | PIIODevice | inline
piCoutObj | PIObject | related
piDisconnect(PIObject *src, const PIString &sig) | PIObject | static
piDisconnect(PIObject *src) | PIObject | static
piHigh enum value | PIThread |
piHighest enum value | PIThread |
PIIODevice() | PIIODevice |
PIIODevice(const PIString &path, DeviceMode mode=ReadWrite) | PIIODevice |
PIIODEVICE | PIIODevice | related
piLow enum value | PIThread |
piLowerst enum value | PIThread |
piNormal enum value | PIThread |
PIObject(const PIString &name=PIString()) | PIObject |
PIOBJECT | PIObject | related
PIOBJECT_SUBCLASS | PIObject | related
PISerial() | PISerial | explicit
PISerial(const PIString &device, PISerial::Speed speed=S115200, PIFlags< PISerial::Parameters > params=0) | PISerial | explicit
PIThread(void *data, ThreadFunc func, bool startNow=false, int loop_delay=-1) | PIThread |
PIThread(bool startNow=false, int loop_delay=-1) | PIThread |
Priority enum name | PIThread |
priority() const | PIThread | inline
properties() const | PIObject | inline
propertiesCount() const | PIObject | inline
property(const PIString &name) const | PIObject | inline
propertyChanged(const PIString &name) | PIObject | inlineprotectedvirtual
read(void *read_to, int max_size) | PISerial | virtual
read(void *read_to, int max_size, double timeout_ms) | PISerial |
read(int size=-1, double timeout_ms=1000.) | PISerial |
PIIODevice::read(int max_size) | PIIODevice | inline
readData(int size=-1, double timeout_ms=1000.) | PISerial |
readDeviceSetting(const PIString &name, const T &def, const PIConfig::Entry *em, const PIConfig::Entry *ep) | PIIODevice | related
readForTime(double timeout_ms) | PIIODevice |
ReadOnly enum value | PIIODevice |
ReadWrite enum value | PIIODevice |
received(const void *data, int size) | PISerial | inlineprotectedvirtual
REGISTER_DEVICE | PIIODevice | related
reopenEnabled | PIIODevice |
reopenTimeout | PIIODevice |
reopenTimeout() | PIIODevice | inline
S1000000 enum value | PISerial |
S110 enum value | PISerial |
S115200 enum value | PISerial |
S1152000 enum value | PISerial |
S1200 enum value | PISerial |
S1500000 enum value | PISerial |
S19200 enum value | PISerial |
S2000000 enum value | PISerial |
S230400 enum value | PISerial |
S2400 enum value | PISerial |
S2500000 enum value | PISerial |
S300 enum value | PISerial |
S3000000 enum value | PISerial |
S3500000 enum value | PISerial |
S38400 enum value | PISerial |
S4000000 enum value | PISerial |
S460800 enum value | PISerial |
S4800 enum value | PISerial |
S50 enum value | PISerial |
S500000 enum value | PISerial |
S57600 enum value | PISerial |
S576000 enum value | PISerial |
S600 enum value | PISerial |
S75 enum value | PISerial |
S921600 enum value | PISerial |
S9600 enum value | PISerial |
send(const void *data, int size, bool wait=false) | PISerial | inline
send(const PIString &data, bool wait=false) | PISerial | inline
send(const PIByteArray &data, bool wait=false) | PISerial | inline
setData(void *d) | PIThread | inline
setDataBitsCount(int bits) | PISerial | inline
setDebug(bool debug) | PIObject | inline
setDevice(const PIString &dev) | PISerial | inline
setInSpeed(PISerial::Speed speed) | PISerial | inline
setMode(DeviceMode m) | PIIODevice | inline
setName(const PIString &name) | PIObject | inline
setOutSpeed(PISerial::Speed speed) | PISerial | inline
setParameter(PISerial::Parameters parameter, bool on=true) | PISerial |
setParameters(PIFlags< PISerial::Parameters > parameters_) | PISerial | inline
setPath(const PIString &path) | PIIODevice | inline
setPin(int number, bool on) | PISerial |
setPriority(PIThread::Priority prior) | PIThread |
setProperty(const PIString &name, const PIVariant &value) | PIObject | inline
setReadIsBlocking(bool yes) | PISerial |
setReopenEnabled(bool yes=true) | PIIODevice | inline
setReopenTimeout(int msecs) | PIIODevice | inline
setSlot(ThreadFunc func) | PIThread | inline
setSpeed(PISerial::Speed speed) | PISerial | inline
setThreadedReadBufferSize(int new_size) | PIIODevice | inline
setThreadedReadData(void *d) | PIIODevice | inline
setThreadedReadSlot(ReadRetFunc func) | PIIODevice | inline
Speed enum name | PISerial |
speed | PISerial |
start() | PIIODevice | inline
PIThread::start(int timer_delay) | PIThread |
PIThread::start(ThreadFunc func, int timer_delay) | PIThread | inline
started() | PIThread |
startOnce() | PIThread |
startOnce(ThreadFunc func) | PIThread | inline
startThreadedRead() | PIIODevice | inline
startThreadedRead(ReadRetFunc func) | PIIODevice | inline
startThreadedWrite() | PIIODevice | inline
stop(bool wait=false) | PIIODevice | inline
stopped() | PIThread |
stopThreadedRead() | PIIODevice | inline
stopThreadedWrite() | PIIODevice | inline
superClassName() const | PIObject | inlinevirtual
threadedRead(uchar *readed, int size) | PIIODevice | inlineprotectedvirtual
threadedReadBuffer() const | PIIODevice | inline
threadedReadBufferSize | PIIODevice |
threadedReadBufferSize() const | PIIODevice | inline
threadedReadData() const | PIIODevice | inline
threadedReadEvent(uchar *readed, int size) | PIIODevice |
threadedWriteEvent(ullong id, int written_size) | PIIODevice |
TwoStopBits enum value | PISerial |
twoStopBits | PISerial |
unlock() | PIThread | inline
waitForFinish(int timeout_msecs) | PIThread |
waitForStart(int timeout_msecs) | PIThread |
WEAK_CONNECT | PIObject | related
WEAK_CONNECT0 | PIObject | related
WEAK_CONNECT1 | PIObject | related
WEAK_CONNECT2 | PIObject | related
WEAK_CONNECT3 | PIObject | related
WEAK_CONNECT4 | PIObject | related
write(const void *data, int max_size, bool wait=false) | PISerial |
write(const void *data, int max_size) | PISerial | inlineprotectedvirtual
PIIODevice::write(const PIByteArray &data) | PIIODevice | inline
WriteOnly enum value | PIIODevice |
writeThreaded(const void *data, int max_size) | PIIODevice | inline
writeThreaded(const PIByteArray &data) | PIIODevice |