# PIP: Member List

PIFile Member List

This is the complete list of members for PIFile, including all inherited members.

applyFileInfo(const PIString &path, const FileInfo &info) | PIFile | static
applyFileInfo(const FileInfo &info) | PIFile | inlinestatic
canRead() const | PIIODevice | inlinevirtual
canWrite() const | PIIODevice | inlinevirtual
className() const | PIObject | inlinevirtual
clear() | PIFile |
clearThreadedWriteQueue() | PIIODevice | inline
close() | PIIODevice | inline
closed() | PIIODevice |
closeDevice() | PIFile | protectedvirtual
configure(const PIString &config_file, const PIString &section, bool parent_section=false) | PIIODevice |
configureDevice(const void *e_main, const void *e_parent=0) | PIIODevice | inlineprotectedvirtual
configureFromFullPath(const PIString &full_path) | PIFile | protectedvirtual
CONNECT | PIObject | related
CONNECT0 | PIObject | related
CONNECT1 | PIObject | related
CONNECT2 | PIObject | related
CONNECT3 | PIObject | related
CONNECT4 | PIObject | related
CONNECTU | PIObject | related
constructFullPath() const | PIFile | virtual
createFromFullPath(const PIString &full_path) | PIIODevice | static
data() const | PIThread | inline
debug() const | PIObject | inline
deleted() | PIObject | protected
DeviceMode enum name | PIIODevice |
DISCONNECT | PIObject | related
DISCONNECT0 | PIObject | related
DISCONNECT1 | PIObject | related
DISCONNECT2 | PIObject | related
DISCONNECT3 | PIObject | related
DISCONNECT4 | PIObject | related
emitter() const | PIObject | inlineprotected
EVENT | PIObject | related
EVENT0 | PIObject | related
EVENT1 | PIObject | related
EVENT2 | PIObject | related
EVENT3 | PIObject | related
EVENT4 | PIObject | related
EVENT_HANDLER | PIObject | related
EVENT_HANDLER0 | PIObject | related
EVENT_HANDLER1 | PIObject | related
EVENT_HANDLER2 | PIObject | related
EVENT_HANDLER3 | PIObject | related
EVENT_HANDLER4 | PIObject | related
EVENT_VHANDLER | PIObject | related
EVENT_VHANDLER0 | PIObject | related
EVENT_VHANDLER1 | PIObject | related
EVENT_VHANDLER2 | PIObject | related
EVENT_VHANDLER3 | PIObject | related
EVENT_VHANDLER4 | PIObject | related
fileInfo() const | PIFile | inline
fileInfo(const PIString &path) | PIFile | static
findByName(const PIString &name) | PIObject | inlinestatic
flush() | PIFile | virtual
fullPathPrefix() const | PIFile | inlineprotectedvirtual
HANDLER | PIObject | related
init() | PIIODevice | inlineprotectedvirtual
initialize() | PIIODevice | inline
isClosed() const | PIIODevice | inline
isEmpty() const | PIFile | inline
isEnd() const | PIFile |
isExists(const PIString &path) | PIFile | static
isOpened() const | PIIODevice | inline
isPropertyExists(const PIString &name) const | PIObject | inline
isReadable() const | PIIODevice | inline
isReopenEnabled() const | PIIODevice | inline
isRunning() const | PIThread | inline
isThreadedRead() const | PIIODevice | inline
isThreadedWrite() const | PIIODevice | inline
isWriteable() const | PIIODevice | inline
lock() | PIThread | inline
mode() const | PIIODevice | inline
mutex() | PIThread | inline
name() const | PIObject | inline
needLockRun(bool need) | PIThread | inline
open() | PIIODevice | inline
open(const PIString &_path) | PIIODevice | inline
open(const DeviceMode &_mode) | PIIODevice | inline
open(const PIString &_path, const DeviceMode &_mode) | PIIODevice | inline
openDevice() | PIFile | protectedvirtual
opened() | PIIODevice |
openTemporary(PIIODevice::DeviceMode mode=PIIODevice::ReadWrite) | PIFile | inlinestatic
operator<<(const char v) | PIFile | inline
operator<<(const PIString &v) | PIFile | inline
operator<<(const PIByteArray &v) | PIFile | inline
operator<<(short v) | PIFile | inline
operator<<(int v) | PIFile | inline
operator<<(long v) | PIFile | inline
operator<<(llong v) | PIFile | inline
operator<<(uchar v) | PIFile | inline
operator<<(ushort v) | PIFile | inline
operator<<(uint v) | PIFile | inline
operator<<(ulong v) | PIFile | inline
operator<<(ullong v) | PIFile | inline
operator<<(float v) | PIFile | inline
operator<<(double v) | PIFile | inline
operator>>(char &v) | PIFile | inline
operator>>(short &v) | PIFile | inline
operator>>(int &v) | PIFile | inline
operator>>(long &v) | PIFile | inline
operator>>(llong &v) | PIFile | inline
operator>>(uchar &v) | PIFile | inline
operator>>(ushort &v) | PIFile | inline
operator>>(uint &v) | PIFile | inline
operator>>(ulong &v) | PIFile | inline
operator>>(ullong &v) | PIFile | inline
operator>>(float &v) | PIFile | inline
operator>>(double &v) | PIFile | inline
path() const | PIIODevice | inline
piCoutObj | PIObject | related
piDisconnect(PIObject *src, const PIString &sig) | PIObject | static
piDisconnect(PIObject *src) | PIObject | static
PIFile() | PIFile | explicit
PIFile(const PIString &path, DeviceMode mode=ReadWrite) | PIFile | explicit
piHigh enum value | PIThread |
piHighest enum value | PIThread |
PIIODevice() | PIIODevice |
PIIODevice(const PIString &path, DeviceMode mode=ReadWrite) | PIIODevice |
PIIODEVICE | PIIODevice | related
piLow enum value | PIThread |
piLowerst enum value | PIThread |
piNormal enum value | PIThread |
PIObject(const PIString &name=PIString()) | PIObject |
PIOBJECT | PIObject | related
PIOBJECT_SUBCLASS | PIObject | related
PIThread(void *data, ThreadFunc func, bool startNow=false, int loop_delay=-1) | PIThread |
PIThread(bool startNow=false, int loop_delay=-1) | PIThread |
pos() const | PIFile |
precision() const | PIFile | inline
priority() const | PIThread | inline
Priority enum name | PIThread |
properties() const | PIObject | inline
propertiesCount() const | PIObject | inline
property(const PIString &name) const | PIObject | inline
propertyChanged(const PIString &name) | PIObject | inlineprotectedvirtual
read(void *read_to, int max_size) | PIFile | virtual
PIIODevice::read(int max_size) | PIIODevice | inline
readAll(void *data) | PIFile |
readAll(bool forceRead=false) | PIFile |
readChar() | PIFile |
readDeviceSetting(const PIString &name, const T &def, const PIConfig::Entry *em, const PIConfig::Entry *ep) | PIIODevice | related
readForTime(double timeout_ms) | PIIODevice |
readLine() | PIFile |
ReadOnly enum value | PIIODevice |
ReadWrite enum value | PIIODevice |
REGISTER_DEVICE | PIIODevice | related
remove() | PIFile |
remove(const PIString &path) | PIFile | static
rename(const PIString &from, const PIString &to) | PIFile | inlinestatic
reopenEnabled | PIIODevice |
reopenTimeout | PIIODevice |
reopenTimeout() | PIIODevice | inline
resize(llong new_size) | PIFile | inline
resize(llong new_size, uchar fill) | PIFile |
seek(llong position) | PIFile |
seekToBegin() | PIFile |
seekToEnd() | PIFile |
seekToLine(llong line) | PIFile |
setData(void *d) | PIThread | inline
setDebug(bool debug) | PIObject | inline
setMode(DeviceMode m) | PIIODevice | inline
setName(const PIString &name) | PIObject | inline
setPath(const PIString &path) | PIFile |
setPrecision(int prec) | PIFile |
setPriority(PIThread::Priority prior) | PIThread |
setProperty(const PIString &name, const PIVariant &value) | PIObject | inline
setReopenEnabled(bool yes=true) | PIIODevice | inline
setReopenTimeout(int msecs) | PIIODevice | inline
setSlot(ThreadFunc func) | PIThread | inline
setThreadedReadBufferSize(int new_size) | PIIODevice | inline
setThreadedReadData(void *d) | PIIODevice | inline
setThreadedReadSlot(ReadRetFunc func) | PIIODevice | inline
size() const | PIFile |
start() | PIIODevice | inline
PIThread::start(int timer_delay) | PIThread |
PIThread::start(ThreadFunc func, int timer_delay) | PIThread | inline
started() | PIThread |
startOnce() | PIThread |
startOnce(ThreadFunc func) | PIThread | inline
startThreadedRead() | PIIODevice | inline
startThreadedRead(ReadRetFunc func) | PIIODevice | inline
startThreadedWrite() | PIIODevice | inline
stop(bool wait=false) | PIIODevice | inline
stopped() | PIThread |
stopThreadedRead() | PIIODevice | inline
stopThreadedWrite() | PIIODevice | inline
superClassName() const | PIObject | inlinevirtual
threadedRead(uchar *readed, int size) | PIIODevice | inlineprotectedvirtual
threadedReadBuffer() const | PIIODevice | inline
threadedReadBufferSize | PIIODevice |
threadedReadBufferSize() const | PIIODevice | inline
threadedReadData() const | PIIODevice | inline
threadedReadEvent(uchar *readed, int size) | PIIODevice |
threadedWriteEvent(ullong id, int written_size) | PIIODevice |
unlock() | PIThread | inline
waitForFinish(int timeout_msecs) | PIThread |
waitForStart(int timeout_msecs) | PIThread |
WEAK_CONNECT | PIObject | related
WEAK_CONNECT0 | PIObject | related
WEAK_CONNECT1 | PIObject | related
WEAK_CONNECT2 | PIObject | related
WEAK_CONNECT3 | PIObject | related
WEAK_CONNECT4 | PIObject | related
write(const void *data, int max_size) | PIFile | virtual
PIIODevice::write(const PIByteArray &data) | PIIODevice | inline
writeBinary(const char v) | PIFile | inline
writeBinary(const short v) | PIFile | inline
writeBinary(const int v) | PIFile | inline
writeBinary(const long v) | PIFile | inline
writeBinary(const llong v) | PIFile | inline
writeBinary(const uchar v) | PIFile | inline
writeBinary(const ushort v) | PIFile | inline
writeBinary(const uint v) | PIFile | inline
writeBinary(const ulong v) | PIFile | inline
writeBinary(const ullong v) | PIFile | inline
writeBinary(const float v) | PIFile | inline
writeBinary(const double v) | PIFile | inline
WriteOnly enum value | PIIODevice |
writeThreaded(const void *data, int max_size) | PIIODevice | inline
writeThreaded(const PIByteArray &data) | PIIODevice |