# PIP: Member List

PIIOString Member List

This is the complete list of members for PIIOString, including all inherited members.

canRead() const | PIIODevice | inlinevirtual
canWrite() const | PIIODevice | inlinevirtual
className() const | PIObject | inlinevirtual
clear() | PIIOString | inline
clearThreadedWriteQueue() | PIIODevice | inline
close() | PIIODevice | inline
closed() | PIIODevice |
closeDevice() | PIIODevice | inlineprotectedvirtual
configure(const PIString &config_file, const PIString &section, bool parent_section=false) | PIIODevice |
configureDevice(const void *e_main, const void *e_parent=0) | PIIODevice | inlineprotectedvirtual
configureFromFullPath(const PIString &full_path) | PIIODevice | inlineprotectedvirtual
CONNECT | PIObject | related
CONNECT0 | PIObject | related
CONNECT1 | PIObject | related
CONNECT2 | PIObject | related
CONNECT3 | PIObject | related
CONNECT4 | PIObject | related
CONNECTU | PIObject | related
constructFullPath() const | PIIODevice | inlinevirtual
createFromFullPath(const PIString &full_path) | PIIODevice | static
data() const | PIThread | inline
debug() const | PIObject | inline
deleted() | PIObject | protected
DeviceMode enum name | PIIODevice |
DISCONNECT | PIObject | related
DISCONNECT0 | PIObject | related
DISCONNECT1 | PIObject | related
DISCONNECT2 | PIObject | related
DISCONNECT3 | PIObject | related
DISCONNECT4 | PIObject | related
emitter() const | PIObject | inlineprotected
EVENT | PIObject | related
EVENT0 | PIObject | related
EVENT1 | PIObject | related
EVENT2 | PIObject | related
EVENT3 | PIObject | related
EVENT4 | PIObject | related
EVENT_HANDLER | PIObject | related
EVENT_HANDLER0 | PIObject | related
EVENT_HANDLER1 | PIObject | related
EVENT_HANDLER2 | PIObject | related
EVENT_HANDLER3 | PIObject | related
EVENT_HANDLER4 | PIObject | related
EVENT_VHANDLER | PIObject | related
EVENT_VHANDLER0 | PIObject | related
EVENT_VHANDLER1 | PIObject | related
EVENT_VHANDLER2 | PIObject | related
EVENT_VHANDLER3 | PIObject | related
EVENT_VHANDLER4 | PIObject | related
findByName(const PIString &name) | PIObject | inlinestatic
flush() | PIIODevice | inlinevirtual
fullPathPrefix() const | PIIODevice | inlinevirtual
HANDLER | PIObject | related
init() | PIIODevice | inlineprotectedvirtual
initialize() | PIIODevice | inline
isClosed() const | PIIODevice | inline
isEnd() const | PIIOString | inline
isOpened() const | PIIODevice | inline
isPropertyExists(const PIString &name) const | PIObject | inline
isReadable() const | PIIODevice | inline
isReopenEnabled() const | PIIODevice | inline
isRunning() const | PIThread | inline
isThreadedRead() const | PIIODevice | inline
isThreadedWrite() const | PIIODevice | inline
isWriteable() const | PIIODevice | inline
lock() | PIThread | inline
mode() const | PIIODevice | inline
mutex() | PIThread | inline
name() const | PIObject | inline
needLockRun(bool need) | PIThread | inline
open(PIString *string, PIIODevice::DeviceMode mode=PIIODevice::ReadWrite) | PIIOString |
open(const PIString &string) | PIIOString |
PIIODevice::open() | PIIODevice | inline
PIIODevice::open(const DeviceMode &_mode) | PIIODevice | inline
PIIODevice::open(const PIString &_path, const DeviceMode &_mode) | PIIODevice | inline
openDevice() | PIIOString | protectedvirtual
opened() | PIIODevice |
path() const | PIIODevice | inline
piCoutObj | PIObject | related
piDisconnect(PIObject *src, const PIString &sig) | PIObject | static
piDisconnect(PIObject *src) | PIObject | static
piHigh enum value | PIThread |
piHighest enum value | PIThread |
PIIODevice() | PIIODevice |
PIIODevice(const PIString &path, DeviceMode mode=ReadWrite) | PIIODevice |
PIIODEVICE | PIIODevice | related
PIIOString(PIString *string=0, PIIODevice::DeviceMode mode=PIIODevice::ReadWrite) | PIIOString |
PIIOString(const PIString &string) | PIIOString |
piLow enum value | PIThread |
piLowerst enum value | PIThread |
piNormal enum value | PIThread |
PIObject(const PIString &name=PIString()) | PIObject |
PIOBJECT | PIObject | related
PIOBJECT_SUBCLASS | PIObject | related
PIThread(void *data, ThreadFunc func, bool startNow=false, int loop_delay=-1) | PIThread |
PIThread(bool startNow=false, int loop_delay=-1) | PIThread |
Priority enum name | PIThread |
priority() const | PIThread | inline
properties() const | PIObject | inline
propertiesCount() const | PIObject | inline
property(const PIString &name) const | PIObject | inline
propertyChanged(const PIString &name) | PIObject | inlineprotectedvirtual
read(void *read_to, int max_size) | PIIOString | virtual
PIIODevice::read(int max_size) | PIIODevice | inline
readDeviceSetting(const PIString &name, const T &def, const PIConfig::Entry *em, const PIConfig::Entry *ep) | PIIODevice | related
readForTime(double timeout_ms) | PIIODevice |
readLine() | PIIOString |
ReadOnly enum value | PIIODevice |
ReadWrite enum value | PIIODevice |
REGISTER_DEVICE | PIIODevice | related
reopenEnabled | PIIODevice |
reopenTimeout | PIIODevice |
reopenTimeout() | PIIODevice | inline
seek(llong position) | PIIOString | inline
seekToBegin() | PIIOString | inline
seekToEnd() | PIIOString | inline
setData(void *d) | PIThread | inline
setDebug(bool debug) | PIObject | inline
setMode(DeviceMode m) | PIIODevice | inline
setName(const PIString &name) | PIObject | inline
setPath(const PIString &path) | PIIODevice | inline
setPriority(PIThread::Priority prior) | PIThread |
setProperty(const PIString &name, const PIVariant &value) | PIObject | inline
setReopenEnabled(bool yes=true) | PIIODevice | inline
setReopenTimeout(int msecs) | PIIODevice | inline
setSlot(ThreadFunc func) | PIThread | inline
setThreadedReadBufferSize(int new_size) | PIIODevice | inline
setThreadedReadData(void *d) | PIIODevice | inline
setThreadedReadSlot(ReadRetFunc func) | PIIODevice | inline
start() | PIIODevice | inline
PIThread::start(int timer_delay) | PIThread |
PIThread::start(ThreadFunc func, int timer_delay) | PIThread | inline
started() | PIThread |
startOnce() | PIThread |
startOnce(ThreadFunc func) | PIThread | inline
startThreadedRead() | PIIODevice | inline
startThreadedRead(ReadRetFunc func) | PIIODevice | inline
startThreadedWrite() | PIIODevice | inline
stop(bool wait=false) | PIIODevice | inline
stopped() | PIThread |
stopThreadedRead() | PIIODevice | inline
stopThreadedWrite() | PIIODevice | inline
string() const | PIIOString | inline
superClassName() const | PIObject | inlinevirtual
threadedRead(uchar *readed, int size) | PIIODevice | inlineprotectedvirtual
threadedReadBuffer() const | PIIODevice | inline
threadedReadBufferSize | PIIODevice |
threadedReadBufferSize() const | PIIODevice | inline
threadedReadData() const | PIIODevice | inline
threadedReadEvent(uchar *readed, int size) | PIIODevice |
threadedWriteEvent(ullong id, int written_size) | PIIODevice |
unlock() | PIThread | inline
waitForFinish(int timeout_msecs) | PIThread |
waitForStart(int timeout_msecs) | PIThread |
WEAK_CONNECT | PIObject | related
WEAK_CONNECT0 | PIObject | related
WEAK_CONNECT1 | PIObject | related
WEAK_CONNECT2 | PIObject | related
WEAK_CONNECT3 | PIObject | related
WEAK_CONNECT4 | PIObject | related
write(const void *data, int max_size) | PIIOString | virtual
PIIODevice::write(const PIByteArray &data) | PIIODevice | inline
WriteOnly enum value | PIIODevice |
writeString(const PIString &string) | PIIOString |
writeThreaded(const void *data, int max_size) | PIIODevice | inline
writeThreaded(const PIByteArray &data) | PIIODevice |